{"text_format":"1","workbook":"xlsx","n_sheets":2,"sheets":["Tabelle1","Tabelle2"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Tabelle1","index":0,"n_rows":24,"n_cols":6,"rows_kept":24,"cut":false,"hidden":false,"merged":[]}
[]
[null,"Geberauswahl","Funktion für Ausgänge","Ausgänge","VBA Elemente "]
[null,"Geber 1","Überdrehzahl","Ausgang zur SPS","weiter"]
[null,"sicherer SinCos-Geber","Unterdrehzahl","sicherer Ausgang zur SPS","zurück"]
[null,"sicherer Inkremental","Frequenzband","Ausgang zu Hilfsrelais"]
[null,"RS422-Geber (A,/A,B,/B)","Stillstand","Ausgang zu Hilfsrelais mit Rückführung (EDM-Funktion)"]
[null,"HTL-Differentiel (A,/A,B,/B)","Drehrichtung"]
[null,"HTL-Geber (A,B,)"]
[null,"Näherungsschalter 3-Leiter PNP"]
[]
[]
[null,"Geber 2","Funktion für Relais","Relais"]
[null,"RS422-Geber (A,/A,B,/B)","Überdrehzahl","Relaisausgang "]
[null,"HTL-Differentiel (A,/A,B,/B)","Unterdrehzahl","Relaisausgang mit Rückführung  (EDM-Funktion)"]
[null,"HTL-Geber (A,B,)","Frequenzband"]
[null,"Näherungsschalter 3-Leiter PNP","Stillstand"]
[null,null,"Drehrichtung"]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,"https://www.excel-vba-lernen.de/13-if-then-else"]

{"sheet":"Tabelle2","index":1,"n_rows":17,"n_cols":5,"rows_kept":17,"cut":false,"hidden":false,"merged":[]}
[]
[null,"Encoder Selection","Function for Outputs","Outputs","VBA Elemente "]
[null,"Encoder 1","Überdrehzahl","Ausgang zur SPS","next"]
[null,"sicherer SinCos-Geber","Unterdrehzahl","sicherer Ausgang zur SPS","back"]
[null,"sicherer Inkremental","Frequenzband","Ausgang zu Hilfsrelais"]
[null,"RS422-Geber (A,/A,B,/B)","Stillstand","Ausgang zu Hilfsrelais mit Rückführung (EDM-Funktion)"]
[null,"HTL-Differentiel (A,/A,B,/B)","Drehrichtung","Relaisausgang "]
[null,"HTL-Geber (A,B,)",null,"Relaisausgang mit Rückführung  (EDM-Funktion)"]
[null,"Näherungsschalter 3-Leiter PNP"]
[]
[]
[null,"Encoder 2","Function for Relais","Relais"]
[null,"RS422-Geber (A,/A,B,/B)","Überdrehzahl","Relaisausgang "]
[null,"HTL-Differentiel (A,/A,B,/B)","Unterdrehzahl","Relaisausgang mit Rückführung  (EDM-Funktion)"]
[null,"HTL-Geber (A,B,)","Frequenzband"]
[null,"Näherungsschalter 3-Leiter PNP","Stillstand"]
[null,null,"Drehrichtung"]